**EPPENDORF CENTRIFUGE INSTRUCTIONS**

**1. Plug the mains plug of the device into a suitable socket and operate the controller using the POWER on the side.**

**2. Open the lid of the device by pressing the lid.**

**3. Weigh your samples in a tube suitable for the rotor (together with the fixing holes), close the rotor and centrifuge caps (Caution: Weights of the samples at the same time for rotor balance).**

**4. Start the centrifugation function using the "Start" button.**

**5. When the centrifugation process is complete (beep sound), wait until speed of rotor becomes “0” , then open the lid.**

**6. Carefully remove your sample from the device.**

**7. If any contamination has occurred on the device or rotor, clean it with a damp cloth or paper towel and close the device cover.**

**8. Sign and fill the device usage notebook.**